**Summary of Speed Indicator Device (SID) Activity**

**For the Period 18th January to 11th February 2021**

**Location :** During this period the SID was positioned on the A 354 Salisbury Road at the East end of the village, which is in a 40 mph speed limit zone.The SID was mounted on a fixed signpost on the left-hand side of the road as you leave Coombe Bissett village heading towards Salisbury. This site is referred to as the Area 1 Secondary site.

For further information regarding approved SID sites in Coombe Bissett and Homington villages please refer to the SID location Power Point guide.

**Detailed PDF reports:**

Please refer to the tab for Salisbury Road for a more detailed analysis of traffic data recorded by the SID, which is presented in PDF report format. Guidance Notes to each section of the PDF reports are provided below this summary.

Note: Our SID does not have GPS and therefore its reports are location agnostic. References in reports to Incoming and Outgoing traffic refer to traffic coming towards the device (Incoming) and traffic going past the device in the opposite direction (Outgoing).

**Period 18th to 29th January 2021**

Location: A354 Salisbury Road, 40 mph speed limit zone. The SID was facing traffic ***coming into*** the village.

|  |  |  |
| --- | --- | --- |
| **Traffic vs. SID** | Towards | Away |
| **Traffic in relation to the village** | Incoming  | Outgoing  |
| Average Speed (mph) | 35.76 | 40.83 |
| Maximum Speed (mph) | 80.00 | 121.00 |
| Traffic Volume (# vehicles) | 22,987 | 22,393 |
| % Less than 46 mph\*  | 91.63 | 78.21 |
| 85th %ile Speed (mph) | 41.00 | 47.00 |

\*Police enforcement in a 40 mph limit is liable at speeds > 46 mph

**Period 2nd to 11th February 2021**

Location: : A354 Salisbury Road, 40 mph speed limit zone. The SID continued to face traffic ***coming into*** the village.

|  |  |  |
| --- | --- | --- |
| **Traffic vs. SID** | Towards | Away |
| **Traffic in relation to the village** | Outgoing  | Incoming |
| Average Speed (mph) | 36.05 | 40.89 |
| Maximum Speed (mph) | 85.00 | 120.00 |
| Traffic Volume (# vehicles) | 20,962 | 20,287 |
| % Less than 46 mph\*  | 91.22 | 77.74 |
| 85th %ile Speed (mph) | 42.00 | 47.00 |

\* Police enforcement in a 40 mph limit is liable at speeds > 46 mph

While the Coombe Bissett Community Speed Watch (CSW) continues to be suspended for the duration of the current Lockdown, we have been advices by Wiltshire CSW in Trowbridge that we can resume speed checks with effect from 29th March 2021.